AGV 4000B is supported through Serial USB interface using AT commands.