AGV 4000 is supported through Serial USB interface using AT commands.
The AGV 4000 is not recommended since it suffers from a bug that limits the functionality. The AGV 4000B does not have that bug.