ElmScan 5 is supported through Serial USB interface using AT commands.