OBD Link SX is supported through Serial USB interface using AT commands.